Cino USB2COM Native Driver for Windows Systems


*Software Revision
Cino_USB2COM Driver_5.0.3.4

*Release Date
 Sep. 23, 2024

*Software Type
 USB2COM Driver

*Description
 The Cino USB virtual COM driver supports FuzzyScan scan engines and scanners. It will create a virtual COM port
 on the host device, enabling the scanner to work as a legacy RS232 serial device. 

 For 2D scanner in "USB HID Mode", a USB serial device also appears in Device Manager. You can send serial command
 to the host without the need of changing the host interface to "USB Com Port Emulation". 
 >> Supported firmware of 2D Scanners: 5.0.19 or above.


*Compatible Devices
 Scan Engines		SE380, SE480, SE6750,SE6850,SE6950
 Scan Module		SM380, SM5800,IM680
 Fixed Mount Scanners	FA490, FA480, FA470, FM490, FM480
 Corded Scanners	A890, A790, A780, A770, A690, A680, A670, A570, A560, F890, F790, F780, L780, F680, L680, F560
 Bluetooth Scanners	A898BT, A798BT, A790BT, A788BT, A780BT, A778BT, A770BT, A698BT, A690BT, A688BT, A680BT, A678BT, A670BT, F898BT, F798BT, F790BT, F788BT, F780BT, F688BT, F680BT, L788BT, L780BT, L688BT, L680BT
 Pocket Scanner		PA680BT, PA670BT, PF680BT, PL680BT
 

*Supported Operating Systems: 
 Windows 7 SP1 32/64 bit, Windows 8 32/64 bit
 For Windows 10 or above, please use native driver included in the Windows operating system.


*Note
If USB2COM Driver version 3.x.x.x had previously been installed, please uninstall it first before installing USB2COM Driver version 5.x.x.x.
For more details, please contact Cino Technical Support.  